DRAWING LINES: Using your steel rule, draw lines of the lengths given below; write the dimension for each line.

a. 1 13/32 in.

b. 3 27/32 in.

c. 5 11/32 in.

d. 4 25/64 in.

e. 1 53/64 in.

f. 16/64 in. (1/4") (Use the 64th in. scale.)